**PCS White Springs Site Safety Requirements That Are Commonly Missed**

**This list does not cover all requirements and is meant only to be a reminder of some of the requirements. Contractor orientation is required with Site Rep. before beginning work.**

1. Emergency Number 8444 (PCS Phone) or 1-386-397-8444 (personal phone)
2. Must have completed Abbottsfield site training prior to reporting
3. Must be clean shaven – no beards in chemical plants
4. Safety Showers / Eyewash identified throughout plant by green lights
5. Plant Fire Extinguishers are identified with red covers
6. Vehicles must have a PCS vehicle pass
7. Vehicles must have company sticker or magnet
8. Vehicles must have an pre-use inspection every shift
9. Obey posted speed limits throughout plant – NO SPEEDING
10. Drivers cannot use cell phones while driving on PCS property – pull over to use phone
11. All occupants in vehicles must wear a seat belt
12. No finger rings
13. When climbing stairs or ladders use 3 point contact – do not skip steps
14. Assume that dripping liquids contain acid – rinse immediately
15. Water used for blasting is reclaimed water – do not drink it or wash with it
16. Plant Restrooms – CLEAN THEM AFTER USING – or we will have to use port-o-lets
17. When putting on rain suits or acid suits – use restroom or PPE trailer – do not dress or undress

 in public areas

1. Goggles or spoggles on person so they are available if needed
2. Barricades must have tags/stickers with – Date – Hazard – Name of

 person erecting barricade

1. Only use approved side grinders (zip cutters)
2. Barricade floors below when working above and possible for falling objects
3. Confined safety monitors/assistants must be trained before being assigned
4. Fire watch must stay with job while assigned and may need to remain after job to make sure fire is out.
5. Safety monitors must wear a safety monitor vest
6. No knives can be used for industrial or construction work
7. LOTO requires tag with – Reason for lock out, Date, Legible first and last name and equipment locked out (equipment number and or name)
8. If you must leave the work area make sure you have removed your lock
9. Everyone must sign on the plant Safe Work Permit and any other plant paperwork

 that applies to the job, read and understand what you are signing

1. Confined Space entrants must be signed in and out and you must understand all applicable rules
2. Report to your crew leader or supervisor immediately any near miss or injury
3. Stop the job and ask questions if you are not sure about what you are doing or if you

 think the job is unsafe

1. All mobile equipment must be equipped with a back up alarm and a charged fire extinguisher that is current on monthly and annual inspection.
2. Work gloves on person at all times when on the job
3. Must complete Job Hazard Analysis (JHA) form